{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["MBIO2IEC104"],"not_rendered":{"macros":1,"comments":1},"read":"whole","date_system":"1900"}

{"sheet":"MBIO2IEC104","index":0,"n_rows":7,"n_cols":31,"rows_kept":7}
[]
[]
["Name","Object Type","Access","Timestamp","Start IOA","Data Quantity","Interrogation Group","Counter Group","IEC104 Data Exchange","Deadband Value","Report Start Type","Interval For Report","Alarm","Alarm Upper Bound","Upper Bound IOA","Alarm Lower Bound","Lower Bound IOA","Local I/O","Modbus Host","Modbus Port","Device ID","Function Code","Modbus Address","Polling Interval","Timeout","Address Bit","Data Type","Data Swap","Byte Swap","Data Multiplier","Data Offset"]
["FC3_A","Bitstring of 32 bit","Read/Write","No time",1,1,0,null,"Send on Request",{"$nulls":3},"No",{"$nulls":5},"192.168.1.102",502,1,3,1,10000,1000,null,"uint32","None","No",1,0]
["FC3_B","Bitstring of 32 bit","Read/Write","No time",2,1,1,null,"Send on Request",{"$nulls":3},"No",{"$nulls":5},"192.168.1.103",502,2,3,1,10000,1000,null,"uint32","None","No",1,0]
["FC3_C","Bitstring of 32 bit","Read/Write","No time",3,1,2,null,"Send on Request",{"$nulls":3},"No",{"$nulls":5},"192.168.1.104",502,3,3,1,10000,1000,null,"uint32","None","No",1,0]
["FC3_D","Bitstring of 32 bit","Read/Write","No time",4,1,3,null,"Send on Request",{"$nulls":3},"No",{"$nulls":5},"192.168.1.105",502,4,3,1,10000,1000,null,"uint32","None","No",1,0]